Button less fobs (Smart FOB)  
  
To view how to deactivate the security system using the manual PIN codes, read here.  
[http://www.hdtalking.com/diagnostics\_alarms\_security\_and\_fuel\_injection\_rel ated/1996-manual\_alarm\_disarming.html](http://www.hdtalking.com/diagnostics_alarms_security_and_fuel_injection_related/1996-manual_alarm_disarming.html)  
  
To view/change the PIN number follow this procedure, but read and understand it first, then see the note at the bottom.  
  
1. Select 5 digit code (1 thru 9) and record it on the wallet card in the owners manual.  
  
2. With an assigned FOB present, turn **IGN** key **ON - OFF - ON - OFF - ON**  
  
3. Press **Left** turn signal switch **2 times**.  
  
4. Press **Right** turn signal switch **one time** and release.  
\*Turn signals will flash **3 times**. Current **PIN** will appear in the odometer. The first digit will be flashing.  
  
5. Enter first digit (**a**) of the new **PIN** by pressing left turn signal (**a**) times.  
  
6. Press right turn signal 1 time and release.  
\*The new digit (**a**) will replace the current in the odometer window.  
  
7. Enter second digit (**b**) of the new **PIN** by pressing **left** turn signal switch (**b**) times.  
  
8. Press right turn signal **1 time** and release.  
\*The new digit will replace the current in odometer window.  
  
9. Enter the third digit (**c**) of the new **PIN** by pressing left turn signal (**c**) times.  
  
10. Press the right turn switch **1 time** and release.  
\*The new digit (**c**) will replace the current in the odometer window.  
  
11. Enter forth digit (**d**) of the new **PIN** by pressing **left** turn signal switch (**d**) times.  
  
12. Press the right turn switch **1 time** and release.  
  
13. Enter the fifth digit (**e**) of the new **PIN** by pressing left turn signal (**e**) times.  
\*The new digit (**e**) will replace the current in the odometer window.  
  
14. Press the right turn switch **1 time** and release.  
  
15. Before the module rearms, turn ignition key to **OFF.**  
\* The odometer will return to mileage display.  
\*\*Turning the ignition to OFF stores the new pin in the module.  
  
NOTE  
The key to doing this proceedure is to turn the ignition switch on/off/on/off/on and use the left directional 3 times then the right just once and do it all in TWO SECONDS or it will not work.  
Also on new installations, the dealer has to program the fob using the bar code for it to work.